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3. Handlungsschritt (25 Punkte)
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) Den Mitarbeitern sall der Zugrif auf das WLAN iber die Authentifizierung nach IEEE 802.1X ermbglicht werden
Dazu liegt Ihnen der folgende englische Text vor:
802.1X authentication involves three parties: a client, an authenticator, and an authentication server.
The client device (e. g. a laptop) wishes to attach to the LANMWIAN. The authenticator fs a network device
(Ethernet switch or wireless access point). The authentication server is typically a RADIUS server.
The authenticator acts like a security quard to a protected network.
The client is ot allowed access through the authenticator to the protected side of the network until the
identity has been validated. With 802.1X port-based authentication, the client provides credentials, such as
user name and password or digital certificate to the authenticator. The authenticator forwards the
credentials to the authentication server for verification.
— If the authentication server determines the credentials are valid, the client is alfowed to access resources

located on the protected side of the network.

~ If the authentication fails, access to resources will be refused.
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be) Erganzen Sie das folgende UML-Sequenzdiagramm in den Punkten 1 7. (14 Punkte)
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